phase-43.42.asc Mon Jul 14 23:50:05 2008 1

CLEAR STORAGE 1     ,008015,022026,030037,044,049,053053N000000N00001026                                         1
CLEAR STORAGE 2     L068116,105106,110117B101/I9I#071029C029056B026/B001/0991,001/001117I0?                      2
BOOTSTRAP           ,008015,022029,036040,047054,061068,072/061039              ,0010011040                      3

                          FORTRAN COMPILER -- SENSE LIGHT PHASE -- PHASE 43                              PAGE    1

 SEQ PG LIN  LABEL  OP    OPERANDS                                            SFX CT  LOCN  INSTRUCTION TYPE  CARD

 101                JOB   FORTRAN COMPILER -- SENSE LIGHT PHASE -- PHASE 43
 102                CTL   6611
 103         *
 104         * IN-LINE INSTRUCTIONS ARE GENERATED.
 105         *
 106         X1     EQU   89                                                          0089
 107         X2     EQU   94                                                          0094
 108         X3     EQU   99                                                          0099
 109         *
 110         * STUFF IN THE RESIDENT AREA
 111         *
 112         PHASID EQU   110  PHASE ID, FOR SNAPSHOT DUMPS                           0110
 113         GLOBER EQU   184  GLOBAL ERROR FLAG -- WM MEANS ERROR                    0184
 114         SNAPSH EQU   333  CORE DUMP SNAPSHOT                                     0333
 115         LOADNX EQU   700  LOAD NEXT OVERLAY                                      0700
 116         CLEARL EQU   707  CS AT START OF OVERLAY LOADER                          0707
 117         CDOVLY EQU   769  1 IF RUNNING FROM CARDS, N IF FROM TAPE                0769
 118         *
 119                ORG   838                                                                0838
 120         LOADDD EQU   *&1          LOAD ADDRESS                                   0838
 121    838  BEGINN BCE   DONE,0&X1,                                               8  0838  B 861 0|0            4
 122    846         MCW   0&X1,SEQCOD                                              7  0846  M 0|0 /88            4
 123    853         BCE   SLITE,SEQCOD-3,J                                         8  0853  B 884 /85 J          4
 124    861  DONE   BSS   SNAPSH,C                                                 5  0861  B 333 C              4
 125    866         SBR   CLEARL&3,GMWM                                            7  0866  H 710 S92            4
 126    873         LCA   IFCOND,PHASID                                            7  0873  L /94 110            5
 127    880         B     LOADNX                                                   4  0880  B 700                5
 128    884  SLITE  LCA   0&X1,0&X3                                                7  0884  L 0|0 0?0            5
 129    891         SAR   X1                                                       4  0891  Q 089                5
 130    895         C     0&X3                                                     4  0895  C 0?0                5
 131    899         SAR   X3                                                       4  0899  Q 099                5
 132    903         SBR   TSTBRK&6,1&X1                                            7  0903  H /26 0|1            5
 133    910         MCW   RBRACK,1&X1                                              7  0910  M /95 0|1            6
 134    917         LCA   1&X3,2&X3                                                7  0917  L 0?1 0?2            6
 135    924         SBR   X3                                                       4  0924  H 099                6
 136    928         MCW   SEQCOD,W3                                                7  0928  M /88 /98            6
 137    935         BWZ   *&5,W3,2                                                 8  0935  V 947 /98 2          6
 138    943         B     *&9                                                      4  0943  B 955                6
 139    947         BWZ   *&15,W3-2,2                                              8  0947  V 969 /96 2          7
 140    955         MCW   W3,X2                                                    7  0955  M /98 094            7
 141    962         MCW   0&X2,W3                                                  7  0962  M 0!0 /98            7
 142    969         BCE   SYNTAX,0&X1,}                                            8  0969  B |15 0|0 } GMARK    7
 143    977         MCW   0&X1,W2                                                  7  0977  M 0|0 S00            7
 144    984         BCE   TSTCOD,W2-1,}  SENSE LIGHT NUMBER IS ONE DIGIT?          8  0984  B 996 /99 } GMARK    8
 145    992         B     SYNTAX                                                   4  0992  B |15                8
 146    996  TSTCOD MN    0&X1,*&8                                                 7  0996  D 0|0 |10            8
 147  1 003         BCE   SENSOK,K01234,0  VALID SENSE LIGHT NUMBER?               8  1003  B |68 S05 0          8

phase-43.42.asc Mon Jul 14 23:50:05 2008 2

                          FORTRAN COMPILER -- SENSE LIGHT PHASE -- PHASE 43                              PAGE    2

 SEQ PG LIN  LABEL  OP    OPERANDS                                            SFX CT  LOCN  INSTRUCTION TYPE  CARD

 148  1 011         CHAIN 4                                                                             MACRO
 149                BCE                                                            1  1011  B           GEN      8
 150                BCE                                                            1  1012  B           GEN      8
 151                BCE                                                            1  1013  B           GEN      8
 152                BCE                                                            1  1014  B           GEN      9
 153  1 015  SYNTAX CS    332                                                      4  1015  / 332                9
 154  1 019         CS                                                             1  1019  /                    9
 155  1 020         SW    GLOBER                                                   4  1020  , 184                9
 156  1 024         MN    W3,245                                                   7  1024  D /98 245            9
 157  1 031         MN                                                             1  1031  D                    9
 158  1 032         MN                                                             1  1032  D                    9
 159  1 033         MCW   ERR36                                                    4  1033  M S47               10
 160  1 037         W                                                              1  1037  2                   10
 161  1 038         BCV   *&5                                                      5  1038  B |47 @             10
 162  1 043         B     *&3                                                      4  1043  B |49               10
 163  1 047         CC    1                                                        2  1047  F 1                 10
 164  1 049         SBR   X3,4&X3                                                  7  1049  H 099 0?4           10
 165  1 056         C     0&X1                                                     4  1056  C 0|0               10
 166  1 060         SAR   X1                                                       4  1060  Q 089               11
 167  1 064         B     BEGINN                                                   4  1064  B 838               11
 168  1 068  SENSOK MZ    *-4,0&X1                                                 7  1068  Y |70 0|0           11
 169  1 075         BCE   SENSE0,0&X1,0                                            8  1075  B /62 0|0 0         11
 170  1 083         MN    0&X1,CW&3                                                7  1083  D 0|0 /84           11
 171  1 090         LCA   CW&3,0&X3  LOAD CW INSTRUCTION                           7  1090  L /84 0?0           11
 172  1 097         SBR   X3                                                       4  1097  H 099               12
 173  1 101  ENDSTM C     0&X1                                                     4  1101  C 0|0               12
 174  1 105         SAR   X1                                                       4  1105  Q 089               12
 175  1 109         LCA   1&X1,0&X3  GMWM                                          7  1109  L 0|1 0?0           12
 176  1 116         SBR   X3                                                       4  1116  H 099               12
 177  1 120  TSTBRK BCE   BEGINN,0,]  NOT TOO BIG IF BRACKET NOT CLOBBERED         8  1120  B 838 000 ]         12
 178  1 128         CS    332                                                      4  1128  / 332               12
 179  1 132         CS                                                             1  1132  /                   13
 180  1 133         CC    1                                                        2  1133  F 1                 13
 181  1 135         MCW   ERROR2,270                                               7  1135  M S83 270           13
 182  1 142         W                                                              1  1142  2                   13
 183  1 143         CC    1                                                        2  1143  F 1                 13
 184  1 145         BCE   HALT,CDOVLY,1                                            8  1145  B /58 769 1         13
 185  1 153         RWD   1                                                        5  1153  U %U1 R             13
 186  1 158  HALT   H     HALT                                                     4  1158  . /58               14
 187  1 162  SENSE0 LCA   SW,0&X3  CHAINED SW                                      7  1162  L S84 0?0           14
 188  1 169         LCA   SW2&6    SW 82,84                                        4  1169  L S91               14
 189  1 173         SBR   X3                                                       4  1173  H 099               14
 190  1 177         B     ENDSTM                                                   4  1177  B /01               14
 191  1 181  CW     CW    80                                                       4  1181  ) 080               14
 192  1 188  SEQCOD DCW   #4                                                       4  1188                      14
 193  1 194  IFCOND DCW   @IFCOND@                                                 6  1194                      15
 194  1 195  RBRACK DCW   @]@                                                      1  1195                      15
 195  1 198  W3     DCW   #3                                                       3  1198                      15
 196  1 200  W2     DCW   #2                                                       2  1200                      15
 197  1 205  K01234 DCW   @01234@                                                  5  1205                      15

phase-43.42.asc Mon Jul 14 23:50:05 2008 3

                          FORTRAN COMPILER -- SENSE LIGHT PHASE -- PHASE 43                              PAGE    3

 SEQ PG LIN  LABEL  OP    OPERANDS                                            SFX CT  LOCN  INSTRUCTION TYPE  CARD

 198  1 247  ERR36  DCW   @ERROR 36 - ILLEGAL SENSE LIGHT, STATEMENT @            42  1247                      17
 199  1 283  ERROR2 DCW   @MESSAGE 2 - OBJECT PROGRAM TOO LARGE@                  36  1283                      17
 200  1 284  SW     SW                                                             1  1284  ,                   18
 201  1 285  SW2    SW    82,84                                                    7  1285  , 082 084           18
 202  1 292  GMWM   DCW   @}@                                                      1  1292              GMARK   18
 203                ORG   201                                                                0201
 204    203         DSA   LOADDD    LOAD ADDRESS FOR CARD-TO-TAPE PROGRAM          3  0203  838                 19
 205                EX    BEGINN                                                            B 838               20
 206                END                                                                     / 000 080

phase-43.42.asc Mon Jul 14 23:50:05 2008 4

                          FORTRAN COMPILER -- SENSE LIGHT PHASE -- PHASE 43                              PAGE    4

SYMBOL  ADDRESS  SYMBOL  ADDRESS  SYMBOL  ADDRESS  SYMBOL  ADDRESS  SYMBOL  ADDRESS  SYMBOL  ADDRESS  SYMBOL  ADDRESS
BEGINN    838    CDOVLY    769    CLEARL    707    CW       1181    DONE      861    ENDSTM   1101    ERR36    1247
ERROR2   1283    GLOBER    184    GMWM     1292    HALT     1158    IFCOND   1194    K01234   1205    LOADDD    838
LOADNX    700    PHASID    110    RBRACK   1195    SENSE0   1162    SENSOK   1068    SEQCOD   1188    SLITE     884
SNAPSH    333    SW       1284    SW2      1285    SYNTAX   1015    TSTBRK   1120    TSTCOD    996    W2       1200
W3       1198    X1         89    X2         94    X3         99