phase-61.312.asc Mon Jul 14 23:50:06 2008 1

CLEAR STORAGE 1     ,008015,022026,030037,044,049,053053N000000N00001026                                         1
CLEAR STORAGE 2     L068116,105106,110117B101/I9I#071029C029056B026/B001/0991,001/001117I0?                      2
BOOTSTRAP           ,008015,022029,036040,047054,061068,072/061039              ,0010011040                      3

                          FORTRAN COMPILER -- GEAUX PHASE ONE -- PHASE 61                                PAGE    1

 SEQ PG LIN  LABEL  OP    OPERANDS                                            SFX CT  LOCN  INSTRUCTION TYPE  CARD

 101                JOB   FORTRAN COMPILER -- GEAUX PHASE ONE -- PHASE 61
 102                CTL   6611
 103         *
 104         * THIS PHASE PRINTS THE END OF COMPILATION MESSAGE, INITIALIZES
 105         * THE SENSE LIGHTS, AND PREPARES THE BRANCH INTO THE OBJECT
 106         * PROGRAM CODING.
 107         *
 108         X1     EQU   89                                                          0089
 109         *
 110         * ADDRESSES IN THE RESIDENT AREA
 111         *
 112         NSTMTS EQU   183  NUMBER OF STATEMENTS, INCLUDING GENERATED STOP         0183
 113         *                 BEGINNING OF CODE BY NOW
 114         GLOBER EQU   184  GLOBAL ERROR FLAG -- WM MEANS ERROR                    0184
 115         GOTXL  EQU   185  XLINKF WAS REFERENCED IF NO WM                         0185
 116         SNAPSH EQU   333  CORE DUMP SNAPSHOT                                     0333
 117         PHASLD EQU   381  LOADS PHASE ID IN SNAPSHOT                             0381
 118         SNAPEX EQU   564  HALT END EXIT IN SNAPSHOT                              0564
 119         CONDNS EQU   693  P FOR CONDENSED DECK                                   0693
 120         LOADNX EQU   700  LOAD NEXT OVERLAY                                      0700
 121         CLEARL EQU   707  CS AT START OF OVERLAY LOADER                          0707
 122         CDOVLY EQU   769  1 IF RUNNING FROM CARDS, N IF FROM TAPE                0769
 123         TPREAD EQU   780  TAPE READ INSTRUCTION IN OVERLAY LOADER                0780
 124         LOADXX EQU   793  EXIT FROM OVERLAY LOADER                               0793
 125         CLRBOT EQU   833  BOTTOM OF CORE TO CLEAR IN OVERLAY LOADER              0833
 126         *
 127                ORG   838                                                                0838
 128    838  BEGINN LCA   W4,84  INITIALIZE                                        7  0838  L |78 084            4
 129    845         SW    84       SENSE                                           4  0845  , 084                4
 130    849         SW               LIGHTS                                        1  0849  ,                    4
 131    850         SW                                                             1  0850  ,                    4
 132    851         CC    1                                                        2  0851  F 1                  4
 133    853         CS    332                                                      4  0853  / 332                4
 134    857         CS                                                             1  0857  /                    4
 135    858         MCW   ENDMSG,218                                               7  0858  M |96 218            5
 136    865         W                                                              1  0865  2                    5
 137    866         MCW   NSTMTS,X1  ENTRY ADDRESS FOR GENERATED CODE              7  0866  M 183 089            5
 138    873         BW    ERRORS,GLOBER                                            8  0873  V |56 184 1          5
 139    881         CC    J                                                        2  0881  F J                  5
 140    883         CS    332                                                      4  0883  / 332                5
 141    887         CS                                                             1  0887  /                    5
 142    888         MCW   START,217                                                7  0888  M /13 217            6
 143    895         W                                                              1  0895  2                    6
 144    896  AFTERR SW    GMWM                                                     4  0896  , /44                6
 145    900         LCA   GMWM,CONDNS  WHY HERE???                                 7  0900  L /44 693            6
 146    907         BCE   CARDS,CDOVLY,1                                           8  0907  B 963 769 1          6
 147    915         BW    SKIPTP,GOTXL                                             8  0915  V 988 185 1          6

phase-61.312.asc Mon Jul 14 23:50:06 2008 2

                          FORTRAN COMPILER -- GEAUX PHASE ONE -- PHASE 61                                PAGE    2

 SEQ PG LIN  LABEL  OP    OPERANDS                                            SFX CT  LOCN  INSTRUCTION TYPE  CARD

 148    923         SBR   RETRY&3,RD333                                            7  0923  H 962 930            7
 149         *
 150         * LOAD OVERLAY LOADER
 151         *
 152    930  RD333  RTW   1,SNAPSH                                                 8  0930  L %U1 333 R          7
 153    938         BER   TAPERR                                                   5  0938  B 947 L              7
 154    943         B     AFTOVL                                                   4  0943  B |20                7
 155    947  TAPERR BSP   1                                                        5  0947  U %U1 B              7
 156    952         H     4444,4444                                                7  0952  . 44U 44U            7
 157    959  RETRY  B     SKIPTP                                                   4  0959  B 988                8
 158    963  CARDS  BW    SKIPLD,GOTXL                                             8  0963  V 975 185 1          8
 159    971         R     40  LOAD OVERLAY LOADER                                  4  0971  1 040                8
 160         *
 161         * SKIP OVERLAY LOADER
 162         *
 163    975  SKIPLD R                                                              1  0975  1                    8
 164    976         BCE   DONE,68,B                                                8  0976  B |01 068 B          8
 165    984         B     SKIPLD                                                   4  0984  B 975                8
 166    988  SKIPTP RTW   1,GMWM                                                   8  0988  L %U1 /44 R          8
 167    996         BER   TAPERR                                                   5  0996  B 947 L              9
 168         *
 169  1 001  DONE   BSS   SNAPSH,C                                                 5  1001  B 333 C              9
 170  1 006         LCA   NOP,PHASLD                                               7  1006  L /14 381            9
 171  1 013         LCA   HALT,SNAPEX                                              7  1013  L /15 564            9
 172         *
 173         * RETURN HERE AFTER LOADING OVERLAY LOADER
 174         *
 175  1 020  AFTOVL CW    680  IN CASE OF OVERLAY LOADER, CLEAR ITS GMWM           4  1020  ) 680                9
 176  1 024         SBR   CLEARL&3,GMWM                                            7  1024  H 710 /44            9
 177  1 031         SBR   TPREAD&6,201                                             7  1031  H 786 201           10
 178  1 038         SBR   LOADXX&3,201                                             7  1038  H 796 201           10
 179  1 045         SBR   CLRBOT,BEGINN                                            7  1045  H 833 838           10
 180  1 052         B     LOADNX                                                   4  1052  B 700               10
 181         *
 182  1 056  ERRORS CC    J                                                        2  1056  F J                 10
 183  1 058         CS    332                                                      4  1058  / 332               10
 184  1 062         CS                                                             1  1062  /                   10
 185  1 063         MCW   ERRMSG,228                                               7  1063  M /43 228           11
 186  1 070         W                                                              1  1070  2                   11
 187  1 071         B     AFTERR                                                   4  1071  B 896               11
 188  1 078  W4     DCW   #4                                                       4  1078                      11
 189  1 096  ENDMSG DCW   @END OF COMPILATION@                                    18  1096                      11
 190  1 113  START  DCW   @PRESS START TO GO@                                     17  1113                      12
 191  1 114  NOP    NOP                                                            1  1114  N                   12
 192  1 115  HALT   H                                                              1  1115  .                   12
 193  1 143  ERRMSG DCW   @CORRECT ERRORS AND RECOMPILE@                          28  1143                      13
 194  1 144  GMWM   DCW   @}@                                                      1  1144              GMARK   13
 195                EX    BEGINN                                                            B 838               14
 196                END                                                                     / 000 080

phase-61.312.asc Mon Jul 14 23:50:06 2008 3

                          FORTRAN COMPILER -- GEAUX PHASE ONE -- PHASE 61                                PAGE    3

SYMBOL  ADDRESS  SYMBOL  ADDRESS  SYMBOL  ADDRESS  SYMBOL  ADDRESS  SYMBOL  ADDRESS  SYMBOL  ADDRESS  SYMBOL  ADDRESS
AFTERR    896    AFTOVL   1020    BEGINN    838    CARDS     963    CDOVLY    769    CLEARL    707    CLRBOT    833
CONDNS    693    DONE     1001    ENDMSG   1096    ERRMSG   1143    ERRORS   1056    GLOBER    184    GMWM     1144
GOTXL     185    HALT     1115    LOADNX    700    LOADXX    793    NOP      1114    NSTMTS    183    PHASLD    381
RD333     930    RETRY     959    SKIPLD    975    SKIPTP    988    SNAPEX    564    SNAPSH    333    START    1113
TAPERR    947    TPREAD    780    W4       1078    X1         89